LazyTurn bombs / kicks you out when you do the  following:
Rough pass
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Gets about here and just closes down the program here
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Was able to duplicate it five times……..

