MOTOR CONNECTIONS
CONNECTIONS FROM SERVO DRIVER “CN2 PINS” INTO THE MOTOR ENCODER  
CN2 PINS: 





MOTOR ENCODER PINS


1 
GND
------------------------------------------------------              7   E0V (encoder 0V)                                                                             

4             +5V
------------------------------------------------------
8   E5V (encoder +5V)

14            S(Z)+
------------------------------------------------------
5   S +

15             S(Z) -
------------------------------------------------------
6   S -



16             A +
------------------------------------------------------             1    A+ 

17             A -      ------------------------------------------------------
2    A-

18             B+      ------------------------------------------------------

3    B+

19             B -     ------------------------------------------------------               4    B -

20             FG (Cable shielded ground [note 1]) -------------                     9   FG

Note:  servo driver user guide Page: 5-21, 5-48,49  
Note B: We have 2x 7711 breakout board and 1x 7535P  digital board   
Connections For Axis: X 

CONNECTIONS FROM SERVO Driver “CN1 pins” INTO THE DSPMC/IP CONTROLLER THROUGH BREAKOUT BOARD   
CN1 PINS: 

                                    Breakout Board               
         DSPMC/IP PINS:   
3 REF  (speed command input)


7711 (a)

15  (J2)  Analogue output 0
4 AGN (speed command input ground) 

7711 (a)

17 (J2)   Ground (return)

14 Run (run command input) 


7535   
  

 14 (J4)    output 0

19 EGND (Encoder output ground)

7711 (b)

 17 (J6)   Ground

20   +A    (Encoder A+ output)


7711 (b)

 1   (J6)      Ch 0 A+

21   - A
(Encoder A- output) 


7711  (b)

 14  (J6)  Ch 0 A-

22   –B    (Encoder B- output)


7711  (b)

 15  (J6)  Ch 0 B-


23  +B  (Encoder B+ output) 


7711  (b)

 2 (J6)  Ch 0 B+

24  +Z  (Encoder Z+ output)


7711 (b)

 3 (J6)   Ch 0  Z+

25   -Z  (Encoder Z - output) 


7711 (b)

 16 (J6) Ch 0 Z-


13 




                +24V

Note:  servo driver user guide pages: 5-9, 13 and DSPMC user guide pages: 13 to 16 on DSPMC)
Connection For Axis: Y 

CONNECTIONS FROM SERVO Driver “CN1 pins”  INTO THE DSPMC/IP CONTROLLER THROUGH BREAKOUT BOARD   
CN1 PINS: 

                                    Breakout Board                       DSPMC/IP PINS: 
3 REF  (speed command input)


7711 (a)

3  (J2) Analogue output 1
4 AGN (speed command input ground) 

7711 (a)

7 (J2) Ground (return)
14 Run (run command input) 


7535   
  

2 (J4)    output 1
19 EGND (Encoder output ground)

7711 (b)

 21 (J6)  Ground (return) 
20   +A    (Encoder A+ output)


7711 (b)

 5   (J6)   Ch 1 A+

21   - A
(Encoder A- output) 


7711  (b)

 18  (J6)  Ch 1 A-

22   –B    (Encoder B- output)


7711  (b)

 19  (J6)  Ch 1 B-


23  +B  (Encoder B+ output) 


7711  (b)

 6 (J6)  Ch 1 B+

24  +Z  (Encoder Z+ output)


7711 (b)

 7 (J6)   Ch 1  Z+

25   -Z  (Encoder Z - output) 


7711 (b)

 20 (J6) Ch 1 Z-


13 




                +24V

Note:  servo driver user guide pages: 5-9, 13 and DSPMC user guide pages: 13 to 16 on DSPMC)
