Hello All,

I have a question / need help on the Motor Tuning Dialog box. I have assembled the following equipment into a test bed as I research the mechanical parts for my router table. Everything is mounted, wired, tested and will actually move when I run the sample programs that came with my copy of Mach 3 (road runner, ball, etc.). I was following the Mach 3 videos by Paul Campbell on YouTube and everything was working fine until the motor tuning section. At this point, I have the tuning points in their default settings (2000, 120, 4, 0.010360, 0, 0). I select X Axis to start tuning, moved the Velocity a nudge, press Save Axis Setting, press Page Up/Down, and get no movement on the X axis, but Y axis moves. Ok, I must have used the wrong pins for the steppers, easy fix. Nope, all axis are terminated in the correct terminals on the BOB. Hmm… go to the Manual control screen to jog things around and X moves as it should. Test Y, Z, A under manual and they work correctly. More hmmm… go back to motor tuning, this time starting with Y and Y moves correctly. Try X, Z, and A, and Y moves. 

So, what am I doing wrong?
(1) CNC.xyz UC100 USB to Parallel CNC Motion Controller
(6) SainSmart CNC Micro-Stepping Stepper Motor Driver 2M542 Bi-polar 2phase 4.2A Switch

(1) Uxcell AC 110V 220V to DC 5V 5A 25W Switch Power Supply Driver

(1) Eyeboot 36V 600W DC Universal Regulated Switching Power Supply AC to DC 16 Amps

(1) SainSmart 5 Axis Breakout Board for Stepper Motor Driver CNC Mill

(6) StepperOnline NEMA 23 CNC Stepper Motor 2.8A 179oz.in 56mm Bipolar for Hobby CNC Kit

(1) Mach 3 Software (came with BOB from SainSmart) Version 3
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